**Introduction to Computer networks**

**Mid Term Exam**

**$ina Rahmany**

* You are required to design a network for class B IP address of 128.0.X.X, in this design you are supposed to have at least one thousand computers in each subnet. (60 marks)
* 128.0.x.x
* we need at least one thousand Hosts= 1000 ==> 2n(power of n)-2 = 1024from(1000)=>n=10host=1022,subnet=64
* 255.255.1111.1100.0000.0000 => subnet= 255.255.252.0=>/22
* Range : 128.0.0.0 - 128.0.3.255
* What is the maximum number of subnets can you have? Demonstrate how you came up with this number.
* host req = 1000 =>2n(power of n)-2=1024from(1000)=>n=10,so num of 0 is 10

zero will start from left and rest will fill by 1 up to 16, so we will have 10

Host = 1022, Subnet=64

Count of 1 from whatever is not zero: Subnet=64

* What would be the subnet mask for this network?

Demonstrate how you came up with this subnet mask. we saw:

255.255.1111 1100. 0000 0000 ,

Subnet = 255.255.252.0

8 + 8 + 6 + 0 = 22 /22

* What would be the IP range of subnet 7? Demonstrate how you came up with the range.
* ranges

first: 128.0.0.0 - 128.0.3.255 3 for 255 – 252 = 3 and 255 for

255 – 0 = 255

second: 128.0.4.0 - 128.0.6.255

thirth: 128.0.7.0 - 128.0.9.255

* seventh: 128.0.19.0 - 128.0.21.255
* Design physical topology, number of connectivity devices and the security of an office with 100 employees where they use an intranet web site (Local web site) where they access company information. Start from the DEMARC point and end at the computer level. Explain why you used the topology that you used. In your design include wireless internet connection. Explain its setup a well. (40 marks)
* for 100 users and hosts and 26 extra ,the ip will be in class C : 200.0.0.0
* host = 100 =>2n-2 = 128 from(100) =>n=7 ,ma host = 126,max subnet=2
* 255.255.255.1000.0000=> subnet = 255.255.255.128 =>25
* range : 200.0.0.0 - 200.0.0.127

200.0.0.128 - 200.0.0.255

Good luck